ROOF DECK
DGN-32 and NN-32

DO MORE WITH LESS USING DGN-32 ROOF DECK

Quickly becoming the industry standard, DGN-32 offers the lowest installed cost with the highest level

3-7/8”

4-1/8”	8”

     	     	  

  3” 

3-7/8”

4-1/8”	8”

of performance,
3”	offering the ultimate

2-1/8”

32”
DGN-32

2-1/8”

32”
NN-32 Nestable

combination of strength
and efficiency.

DGN-32 & NN-32 provide designers section properties and diaphragm shear values for a variety of structural roof applications.
DGN-32 roof deck has been fully evaluated for use with the DeltaGrip® attachment system.

DGN-32 & NN-32 roof deck have natural trapezoidal shapes and inherent shadow ribs.
Avoids the “box” look of many common N roof deck products.
Offers an aesthetically pleasing appearance suitable for many architectural exposed roof deck applications.
DGN-32 & NN-32’s trapezoidal shapes keep the “nested” roof deck from wedging in bundles, giving contractors
better ease of separation and easier placement of deck for safer jobsite conditions.

DGN-32 & NN-32 roof deck are available in several options:
Nestable configuration for screwable sidelaps
Acoustical (Web and total perforation)
DGNF-32 Cellular (See Back)
DGNF-32A Cellular Acoustical (See Back)
Also available as composite floor deck
800-726-2727

www.ascsteeldeck.com

CELLULAR ROOF DECK
DGNF-32

Quickly becoming the industry standard, DGNF-32 offers the lowest installed cost

DO MORE WITH LESS USING DGNF-32 ROOF DECK

with the highest  level of performance, offering the ultimate combination  of strength and efficiency.

3-7/8”

4-1/8”	8”

2-1/8”

32”

 		 	

DGNF-32

3”

ACUSTADEK®
(Acoustical perforated pan option)
DGNF-32A

DGNF-32 provides designers section properties and diaphragm shear values for a variety of structural roof applications.
DGNF-32 roof deck has been fully evaluated for use with the DeltaGrip® attachment system. DGNF-32 roof deck has a flat pan underside hiding the ribs.
Offers an aesthetically pleasing appearance suitable for many architectural exposed roof deck applications.
Non-perforated pan for smooth finish.
Acoustical perforated pan option, contact ASC Steel Deck for acoustical performance.

Contact your
Sales Representative today

All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
©2019 ASC Profiles LLC. All rights reserved. 0119 (PS271) 50

800-726-2727
www.ascsteeldeck.com