3WxH-36

A PROVEN STRUCTURAL DECK PANEL TO DESIGN WITH CONFIDENCE
ASC Steel Deck is committed to providing the highest quality products and services

 	12" 	

3"

36"

4½"

4½"

 	12" 	

3"

36"

4½"

4½"

in the steel deck industry. With extensive independent testing
by an accredited

3WxH-36 Profile

3WxHF-36 Profile

third party, we ensure our products comply

3WxH-36 is our third generation composite floor deck designed
with a 4½" lower flute dimension. 3WxH-36 is the proven work horse for 10' to 14' foot span conditions and meets SDI 3" x 12" standard profile requirements.
Features and Benefits:
50 ksi deck yield strength
Available in G60 and G90 galvanized
Factory applied Prime Shield® prime painted colors in gray and white applied to underside of steel deck
Optimized for DeltaGrip® structural side seam attachment system
Contact us for more information
800-726-2727

All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
©2019 ASC Profiles LLC. All rights reserved. 0119 50 (PS276)

with today’s stringent building codes.

www.ascsteeldeck.com