DELTAGRIP
^®	DG4^TM

Daily Maintenance - Lubrication Points
Proper lubrication of the tool through the 7 Grease Zerk Fittings should be performed as daily maintenance.

^Front ^View	Back View

DELTAGRIP
DG4^TM

^®®

7 Grease Zerk Fittings

45 Degree Grease Zerk (1)

Grease Zerk (2 + 3)

Grease Zerk (6)

Grease Zerk (7)

Grease Zerk (4 + 5)

Please note that daily maintenance of this tool is required and is the responsibility of the tool user. Failure to do so can dam- age the shoulder screw, shackle pin, jaw, and frame. The renter of this tool (ASC Steel Deck Customer) will be responsible for all costs associated with the repair or replacement of damaged parts up to the value of complete tool replacement.

ASC Steel Deck
220 W. Kalama River Rd. Kalama, WA, 98625
800.726.2727

ASCSD-CS-F-7-504 – Updated June 2023